The Draft ICNIRP HF exposure guidelines appear to have removed the reference level limits requirements for instantaneous exposure, i.e. not exceeding 1000 times (power density) the time-averaged reference levels (frequency above 10MHz).

Is this no longer a requirement?